KX3 Menu Commands

hit the N and then key in the menu number and hit Enter.
To read the value now just hit Enter or
To change the value enter the 3 digit value to use and then hit Enter

In this list :-
The first number is the command always 3 digits.
The other numbers are those returned by the program or used to set the menu item, also 3 digits.

Some Menu Commands are read only.

2M Mode
147   000=Not installed  001=Normal  002=Sleep0.25  003=Sleep0.5  004=Sleep0.75  005=Sleep1.0
ACC2 IO
141   000=off  001=on  002=Lo PTT  003=Hi PTT  004=Lo=inh tx  005=hi inh TX
AF Limit
047   001 to 030 (30 is normal)
AFX MD
105   000=off  001=Delay  002=Pitch
AGC MD
128   000=off  001=on
AGC Threshold
074   004 to 008
AGC SPD
129   000=slow  001=Fast
AM Mode
126   000=off  064=On
ATU Data
112   000=Set 1  008=Set 2
ATU MODE
023   000=Not inst  001=BYpass  002=Auto   003 to 010=Test L1 to L8  011 to 018=Test C1 to C8  19=Test CT
AutoOff
133   001=5  002=10 up to 020=100 or 021=Infinite
Battery Charge
137   000=Not Inst  001=Charge Off  002=4Hours  003=8Hours  004=12Hours  005=16Hours
Back Light
138   000=off  001=on
Battery Minimum
024   082=8.2v up to 130=13.0Volts
CW Iambic
001   000=A  128=B
CW Key 1
120   000=Tip Dot  001=Tip Dash  002=Hand
CW Key 2
121   000=Left is dot  016=Left is dash  032=Hand
CW Weight
012   007=1  up to 012=1.25    .05 steps
FM Mode
018   000=off  128=on
LED Brightness
145   0=level 1  to 007=Level 8
Mic Bias
135   000=off  016=on
Mic Button
082   000=off  001=PTT  005=PTT+Up/Dwn
MSG Repeat
005   000 to 255
Oscillator Temperature
206   xx in degrees C
PA Temperature
205   xx in degrees C
Preamp
136   001=10db  002=20db  003=30db
RPT OFS
007   0Khz=000  Other values offset/20  so for example 030 is 600Khz
RX Filter
134   000= Not installed  002=Normal
RX I/Q
123   000=off  004=On
RX SBNL
125   000 to 254
Supply Current
204   x.xxx Amps
Time
201   Time hh:mm:ss
Tune Power
058   000=Normal  001=0.1Watts up to 100=10 Watts   steps of 0.1 Watts
TX Delay
016
TX Gate
101  000  (Always off)
TX SBNUL
127   000 to 250
VFO B Frequency
200   VFO B Frequency
VFO CRS
104   000=0.1  004=0.5  008=1.0  012=2.5   
Vox GN
010   000 to 060
Vox Inhibit
122   000 to 060
Watt Meter
088  007  to 115  (007=0.70  and 115=1.15)
Supply Voltage
k3=204  kx2=202  kx3=202 (read only)
Battery voltage
kx3=203  (read only)
